[11A] ENGINE MECHANICAL <4G6-SOHC> - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL INFORMATION
Item | 4G63 | 4G64
--- | --- | ---
Total displacement mL | 1,997 | 2,351
Bore × Stroke mm | 85 × 88 | 86.5 × 100
Compression ratio | 9.5 | 9.0
Compression chamber | Pentroof
Camshaft arrangement | SOHC
Number of valve | Intake | 8
Exhaust | 8
Valve timing | Intake opening | BTDC 11° | BTDC 16°
Intake closing | ABDC 53° | ABDC 53°
Exhaust opening | BBDC 63° | BBDC 50°
Exhaust closing | ATDC 21° | ATDC 16°
Fuel system | Electronically controlled multipoint fuel injection
Rocker arm | Roller type
Auto-lash adjuster | Equipped

[11A] ENGINE MECHANICAL <4G6-SOHC> - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation