[1] BODY CONSTRUCTION - - SILENCER APPLICATION LOCATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SILENCER APPLICATION LOCATIONS A silencer (MD-12, RSS and melting sheet) has been adhered on the top part of the floor to improve anti-vibration performance and to shut-out exhaust gas heat. NOTE: MD-12 is a high performance sheet composed of asphalt applied with mica and thermosetting resin for improving anti-vibration performance. RSS (Rubber Special Sheet) is a product name of Nihon Tokushu Toryo Co., Ltd. The product features the same performance as a steel sheet sandwich type and refers to a heat cured resin sheet that is molded into a sheet with a uniform thickness (2.0mm). It contains degenerating resin and filler with asphalt and rubber as the main contents.

[1] BODY CONSTRUCTION - - SILENCER APPLICATION LOCATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation