[54C] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Hong Kong spec.> - - TROUBLESHOOTING - HOW TO CONNECT THE SWS MONITOR | PRINT PAGE / INDEX / PRIOR / NEXT

| HOW TO CONNECT THE SWS MONITOR CAUTION Always turn the ignition switch to the "LOCK" (OFF) position before connecting or disconnecting the SWS monitor and the MUT-II/III.
| HOW TO CONNECT THE SWS COMMUNICATION LINE <SWS MONITOR HARNESS (FOR COLUMN-ECU)>
| Remove the steering column cover. Remove the steering column switch connector. Connect the SWS monitor harness (for column-ECU).
| HOW TO CONNECT THE SWS COMMUNICATION LINE <SWS MONITOR HARNESS (FOR 13-PIN CONNECTOR)>
| Connect the SWS monitor harness (for 13-pin connector) to the diagnosis connector (13-pin connector).
| HOW TO ESTABLISH COMMUNICATION BETWEEN DOORS
| Connect special tool SWS monitor harness MB991812 to special tool Door communication adapter harness MB991896. Connect special tool Probe harness MB991822 to the door communication adapter harness assembled in step 1. Confirm that all the harnesses are connected. Then insert the probe of the probe harness to each female connector terminal on the door communication line by backprobing. NOTE: For the connectors and their terminal numbers on the door communication line for the probe to insert, refer to the reference table.
| Reference table of connectors and their terminal numbers on door communication line Insert the probe of the probe harness to each female connector terminal on the door communication line by backprobing.
Connector name | Connector number | Terminal No.
--- | --- | ---
Intermediate connector | Instrument panel wiring harness and floor wiring harness (RH) combination | C-13 (Floor wiring harness (RH) side) | 6
Instrument panel wiring harness and front door wiring harness (RH) combination | C-30 (Front door wiring harness (RH) side) | 13
Instrument panel wiring harness and front door wiring harness (LH) combination | C-33 (Front door wiring harness (LH) side) | 13
Instrument panel wiring harness and floor wiring harness (LH) combination | C-117 (Instrument panel wiring harness side) | 19
Floor wiring harness (RH) and rear door wiring harness (RH) combination | D-02 (Floor wiring harness (RH) side) | 7
Floor wiring harness (LH) and rear door wiring harness (LH) combination | D-26 (Floor wiring harness (LH) side) | 7
Rear door wiring harness (LH) and rear door sub wiring harness (LH) combination | E-09 (Rear door wiring harness (LH) side) | 6
Rear door wiring harness (RH) and rear door sub wiring harness (RH) combination | E-27 (Rear door wiring harness (RH) side) | 6
Front door wiring harness (RH) and front door sub wiring harness (RH) combination | E-29 (Front door wiring harness (RH) side) | 1
Front door wiring harness (LH) and front door sub wiring harness (LH) combination | E-30 (Front door wiring harness (LH) side) | 6
Power window main switch | E-05 | 11
Power window sub switch (front, LH) | E-31 | 6
Power window sub switch (rear RH) | E-21 | 6
Power window sub switch (rear LH) | E-01 | 6

[54C] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Hong Kong spec.> - - TROUBLESHOOTING - HOW TO CONNECT THE SWS MONITOR | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation