[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - EVAPORATIVE EMISSION CONTROL SYSTEM - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION
<4G63, 4G64, 4G69 EXCEPT FOR BRAZIL AND CHILE>
Pre-removal and Post-installation Operation Air Cleaner Cover and Air Intake Hose Removal and Installation (Refer to GROUP 15 - Air Cleaner <4G63-SOHC, 4G64-SOHC>, <4G69>). Battery and Battery Tray Removal and Installation. <4G63-DOHC>
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Purge hose connection
|  | 2. | Vapour hose
|  | 3. | Vent connector
|  | 4. | Vapour hose
|  | 5. | Hose clamp
|  | 6. | Canister
|  | 7. | Fuel high-pressure hose clamp
|  | 8. | Canister bracket
<4G69 VEHICLES FOR BRAZIL AND CHILE>
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Vent hose A
|  | 2. | Vent hose B
|  | 3. | Vent hose C
|  | 4. | Vent pipe assembly
|  | 5. | Evaporative emission ventilation solenoid valve connector
|  | 6. | Onboard refuelling vapour recover (ORVR) vent valve module
|  | 7. | Evaporative emission ventilation solenoid valve
|  | 8. | Purge hose B
|  | 9. | Vapour hose
|  | 10. | Canister and canister bracket assembly
|  | 11 | Canister
|  | 12 | Canister bracket

[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - EVAPORATIVE EMISSION CONTROL SYSTEM - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation