[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T KEY INTERLOCK AND SHIFT LOCK MECHANISMS> - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 6: The ignition key cannot be turned to the LOCK (OFF) position when the selector lever is at the P position. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 6: The ignition key cannot be turned to the LOCK (OFF) position when the selector lever is at the P position.
COMMENTS ON TROUBLE SYMPTOM The cause is probably a malfunction of the selector lever assembly, key interlock cable or ignition key cylinder lock bar.
Possible causes Malfunction of selector lever assembly Malfunction of key interlock cable Malfunction of lock bar
DIAGNOSIS Check by referring to the possible causes.

[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T KEY INTERLOCK AND SHIFT LOCK MECHANISMS> - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 6: The ignition key cannot be turned to the LOCK (OFF) position when the selector lever is at the P position. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation