[42] BODY - - KEYLESS ENTRY SYSTEM - TRANSMITTER - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

TRANSMITTER

DISASSEMBLY AND REASSEMBLY
Post-installation operation Transmitter operation check
|  |  | Disassembly steps
--- | --- | --- | ---
|  | 1. | Screw
|  | 2. | Upper cover
|  | 3. | Transponder <Vehicles with immobiliser>
|  | 4. | Transmitter assembly
<<A>> | >>A<< | 5. | Battery
|  | 6. | Master key
| DISASSEMBLY SERVICE POINT
| <<A>> BATTERY REMOVAL CAUTION Do not allow water or dust to enter the inside of the transmitter assembly when it is open. Also, do not touch the precision electronic device.
| REASSEMBLY SERVICE POINT
| >>A<< BATTERY INSTALLATION CAUTION Do not allow water or dust to enter the inside of the transmitter assembly when it is open. Also, do not touch the precision electronic device.
| Install a new battery to the transmitter assembly with its (+) side facing towards the upper cover side. Battery required for replacement: Coin type battery CR1616

[42] BODY - - KEYLESS ENTRY SYSTEM - TRANSMITTER - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation