[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - SYMPTOM PROCEDURES - ELECTRIC RETRACTABLE REMOTE CONTROLLED DOOR MIRROR - INSPECTION PROCEDURE I-3: Electric retractable remote controlled door mirror timer function does not at all. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE I-3: Electric retractable remote controlled door mirror timer function does not at all.
| CAUTION Whenever the ECU is replaced, ensure that the input and output signal circuits are normal.
| COMMENTS ON TROUBLE SYMPTOM If the door mirror can be folded and unfolded with the remote controlled mirror switch (fold/unfold switch), the ETACS-ECU may be defective.
| POSSIBLE CAUSES Malfunction of the driver’s door switch Malfunction of the ETACS-ECU Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. Check the electric folding door mirrors operation. Check that the door mirror is folded and unfolded with the remote controlled mirror switch when the ignition switch is at ACC position. Q: Is the check result normal? YES: Go to Step 2. NO: Refer to inspection procedure I-1 "Electric retractable remote controlled door mirrors does not work at all."
| Step 2. Pulse check Check the input signals below which are related to the electric retractable remote controlled door mirror timer function.
System switch | Check conditions
--- | ---
Ignition switch (ACC) | When turned from the LOCK (OFF) position to the ACC position
Driver’s door switch | When the driver’s door is opened
OK: The MUT-II/III sounds or the voltmeter needle fluctuates. Q: Are the check result normal? All the signals are received normally.: Go to Step 3. The ignition switch (ACC) signal is not received.: Refer to inspection procedure P-1 "The ignition switch (ACC) signal is not received ." The driver’s door switch signal is not received.: Refer to inspection procedure P-4 "The driver’s door switch signal is not received ."
| Step 3. Retest the system. Check that the electric-folding door mirror timer function works normally. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the ETACS-ECU.

[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - SYMPTOM PROCEDURES - ELECTRIC RETRACTABLE REMOTE CONTROLLED DOOR MIRROR - INSPECTION PROCEDURE I-3: Electric retractable remote controlled door mirror timer function does not at all. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation