[27B] REAR AXLE <4WD> - - ON-VEHICLE SERVICE - WHEEL BEARING AXIAL PLAY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| WHEEL BEARING AXIAL PLAY CHECK For vehicles with drum brake, remove the brake drum. For vehicles with disc brake, remove the caliper assembly, and suspend the caliper assembly with a wire and remove the brake disc.
| Fit the dial gauge as shown in the diagram and move the hub in the axial direction to measure the play. Limit: 0.05 mm If the play exceeds the limit, the drive shaft nut should be tightened to the specified torque and check the axial play again. Tightening torque: 245 ± 29 N·m Replace the wheel bearing if adjustment cannot be made to within the limit. (Refer to GROUP 34-Trailing Arm.)

[27B] REAR AXLE <4WD> - - ON-VEHICLE SERVICE - WHEEL BEARING AXIAL PLAY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation