[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - THROTTLE BODY ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

THROTTLE BODY ASSEMBLY

REMOVAL AND INSTALLATION
Pre-removal Operation Engine Coolant Draining (Refer to GROUP 14, On-vehicle Service - Engine Coolant Replacement ). Intercooler Assembly and Intercooler Outlet Air Hose Removal <4G63-DOHC> (Refer to GROUP 15, Intercooler ). Air Cleaner Removal (Refer to GROUP 15, Air Cleaner <4G63-SOHC, 4G64-SOHC>, <4G63-DOHC>). | Post-installation Operation Air Cleaner Installation (Refer to GROUP 15, Air Cleaner <4G63-SOHC, 4G64-SOHC>, <4G63-DOHC>). Engine Coolant Supplying (Refer to GROUP 14, On-vehicle Service - Engine Coolant Replacement ). Accelerator Cable Adjustment (Refer to GROUP 17, On-vehicle Service - Accelerator Cable Adjustment ). Intercooler Assembly and Intercooler Outlet Air Hose Installation <4G63-DOHC> (Refer to GROUP 15, Intercooler ).
|  |  | REMOVAL STEPS
--- | --- | --- | ---
|  | 1. | Accelerator cable connection
|  | 2. | Throttle position sensor connector
|  | 3. | Idle speed control servo connector
|  | 4. | Water return hose connection
|  | 5. | Water feed hose connection
|  | 6. | Emission vacuum hose connection
|  | 7. | Throttle body assembly
| >>A<< | 8. | Throttle body gasket
| INSTALLATION SERVICE POINT
| >>A<< THROTTLE BODY GASKET INSTALLATION CAUTION Poor idling etc. may result if the throttle body gasket is installed incorrectly.
| Install the throttle body gasket as shown in the illustration.

[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - THROTTLE BODY ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation