[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - TROUBLESHOOTING - DATA LIST REFERENCE TABLE | PRINT PAGE / INDEX / PRIOR / NEXT

DATA LIST REFERENCE TABLE The following items can be read by the MUT-II/III from the ABS-ECU input data.
When the system is normal.
Item No. | Check item | Checking requirements | Normal valve
--- | --- | --- | ---
11 | Front-right ABS sensor | Perform a test run | Vehicle speeds displayed on the speedometer and MUT-II/III are identical.
12 | Front-left ABS sensor
13 | Rear-right ABS sensor
14 | Rear-left ABS sensor
21 | ABS-ECU power supply voltage | Ignition switch: ON | 10 - 16 V
32 | G-sensor output voltage <4WD> | When vehicle is stationary (level) | 2.4 - 2.6 V
When vehicle is being driven | 1.0 - 4.0 V
36 | Stoplight switch | Depress the brake pedal. | ON
Release the brake pedal. | OFF
When the ABS-ECU shut off ABS operation. When the diagnosis system stops the ABS-ECU, the MUT-II/III display data will be unreliable.

[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - TROUBLESHOOTING - DATA LIST REFERENCE TABLE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation