[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - TROUBLESHOOTING - INSPECTION CHART FOR DIAGNOSIS CODE | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION CHART FOR DIAGNOSIS CODE
Code No. | Diagnosis item | Reference page
--- | --- | ---
P0100 | Air flow sensor system |
P0105 | Barometric pressure sensor system <DOHC> |
P0110 | Intake air temperature sensor system |
P0115 | Engine coolant temperature sensor system |
P0120 | Throttle position sensor system |
P0130 | Oxygen sensor (front) system <SOHC> |
P0130 | Oxygen sensor system <DOHC> |
P0135 | Oxygen sensor heater (front) system <SOHC> |
P0135 | Oxygen sensor heater system <DOHC> |
P0136 | Oxygen sensor (rear) system <SOHC> |
P0141 | Oxygen sensor heater (rear) system <SOHC> |
P0170 | Abnormal fuel system <SOHC> |
P0170 | Abnormal fuel system <DOHC> |
P0201 | No.1 Injector system |
P0202 | No.2 Injector system |
P0203 | No.3 Injector system |
P0204 | No.4 Injector system |
P0300 | Ignition coil (power transistor) system |
P0325 | Detonation sensor system |
P0335 | Crank angle sensor system |
P0340 | Camshaft position sensor |
P0400 | Exhaust gas recirculation (EGR) system <SOHC> |
P0400 | Exhaust gas recirculation (EGR) system<DOHC> |
P0403 | Exhaust gas recirculation (EGR) control solenoid valve system |
P0500 | Vehicle speed signal system |
P0622 | Alternator FR terminal system |
P1603 | Battery backup line system |
NOTE: Do not replace the engine -A/T-ECU until a through terminal check reveals there are no short/open circuit. Check that the engine-A/T-ECU earth circuit is normal before checking for the cause of the problem.

[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - TROUBLESHOOTING - INSPECTION CHART FOR DIAGNOSIS CODE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation