[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - FRONT IMPACT SENSORS - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION
| WARNING If a dent, crack, deformation or rust is detected, replace with a new sensor. Check the front impact sensor for dents, cracks, deformation or rust.
| WARNING Always replace the sensor with a new one if the resistance shows a short or open circuit. Check short or open circuit between the terminals of the front impact sensor. When short circuit: 1 Ω or less When open circuit: 2 MΩ or more Check the continuity between the terminal and bracket. If there is a continuity, the insulation is malfunctioned, and replace the sensor with a new one. Check the head lamp support pane for deformation and rust.

[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - FRONT IMPACT SENSORS - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation