[23A] AUTOMATIC TRANSMISSION (FF) - - ON-VEHICLE SERVICE - TRANSFER OIL LEVEL CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| TRANSFER OIL LEVEL CHECK
| Remove the filler plug. Check that the oil level is up to the lower edge of the filler plug hole. Check that the oil is not noticeably dirty. Tighten the filler plug to the specified torque. Tightening torque: 32 ± 2 N·m

[23A] AUTOMATIC TRANSMISSION (FF) - - ON-VEHICLE SERVICE - TRANSFER OIL LEVEL CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation