[23] AUTOMATIC TRANSMISSION - - A/T FLUID COOLER - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

A/T FLUID COOLER

GENERAL INFORMATION The conventional water-cooled (integrated in the radiator) A/T fluid cooler is adopted. For 4G64, 4G69 and 4G63-DOHC, the air-cooled A/T fluid cooler is added to increase the cooling capacity. In addition, for 4G63-DOHC, the A/T fluid cooler guide is installed to provide efficient air delivery to the A/T fluid cooler. CONSTRUCTION DIAGRAM

[23] AUTOMATIC TRANSMISSION - - A/T FLUID COOLER - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation