[51] EXTERIOR - - RADIATOR GRILLE - REMOVAL AND INSTALLATION <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <2400>
|  |  | Removal steps
--- | --- | --- | ---
<<A>> |  | 1. | Clips
| >>A<< | 2. | Radiator grilles
| REMOVAL SERVICE POINT
| <<A>> CLIPS REMOVAL
| To remove the clips from the radiator grille gently pull forward the radiator grille, and use a flat-tipped screwdriver to hold the claw of the clip in the direction of the arrow.
| INSTALLATION SERVICE POINT
| >>A<< RADIATOR GRILLE INSTALLATION Install the radiator grille with the clips installed.

[51] EXTERIOR - - RADIATOR GRILLE - REMOVAL AND INSTALLATION <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation