[54A] CHASSIS ELECTRICAL - - HEADLAMP - HEADLAMP - REMOVAL AND INSTALLATION <2000> | PRINT PAGE / INDEX / PRIOR / NEXT

HEADLAMP

REMOVAL AND INSTALLATION <2000>
Post-installation Operation Headlamp Aiming Adjustment (Refer to ).
|  |  | Removal
--- | --- | --- | ---
<<A>> |  | 1. | Headlamp assembly
CAUTION Before the discharge headlamp is removed and installed, read the troubleshooting thoroughly.
|  |  | Removal steps
--- | --- | --- | ---
|  | • | Front bumper assembly (Refer to GROUP 51, Front bumper assembly ).
|  | 1. | Headlamp body
|  | 2. | Socket cover
<<B>> |  | 3. | Discharge headlamp connector
|  | 4. | Discharge headlamp controller
|  | 5. | Headlamp bulb
| REMOVAL SERVICE POINT
| <<A>> HEADLAMP ASSEMBLY REMOVAL
| Remove half of the front bumper assembling clips and bolts. NOTE: The figure illustrates the procedures to remove the headlamp assembly (LH). Slide the front bumper down to remove the headlamp assembly.
| <<B>> DISCHARGE HEADLAMP CONNECTOR REMOVAL
| Remove the position lamp bulb, and tie a rope to the end of the controller connector and pull it towards the bulb side.

[54A] CHASSIS ELECTRICAL - - HEADLAMP - HEADLAMP - REMOVAL AND INSTALLATION <2000> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation