[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - TROUBLE SYMPTOM CHART | PRINT PAGE / INDEX / PRIOR / NEXT

TROUBLE SYMPTOM CHART
Symptom | Inspection procedure number | Reference page
--- | --- | ---
Communication with the MUT-II/III is not possible. | A-1 |
When the ignition switch is at the LOCK (OFF) position, the functions do not work normally. | A-2 |
Check the battery power supply circuit to the ETACS-ECU.
<FUNCTION SYSTEM>
Symptom | Inspection procedure number | Reference page
--- | --- | ---
Alarm Functions | Ignition key reminder buzzer function does not work. | B-1 |
Lamp reminder buzzer function does not work normally. | B-2 |
R (reverse) position warning function does not work. | B-3 |
Door-ajar warning function does not work. | B-4 |
Turn-signal lamp operation sound function does not work normally. | B-5 |
Downshift inhibitor buzzer does not work normally. <2000-5A/T> | B-6 |
Central door locking system | Central door locking system does not work. | C-1 |
A door or a tailgate can not be locked or unlocked by the central door locking system. | C-2 |
The ignition key reminder function does not work normally. | C-3 |
The impact detection door unlock function does not function. | C-4 |
Power windows | Power windows do not work at all. | D-1 |
Driver's power window does not work by means of the power window main switch. | D-2 |
Relevant power window(s) do not work by means of the front and rear passenger's power window sub switches. | D-3 |
Front and/or rear passenger's power window(s) do not work by means of the power window main switch. | D-4 |
The power window timer function does not work normally. | D-5 |
The window glass lowers automatically while it is rising. | D-6 |
Power window anti-trap function does not work normally. | D-7 |
Keyless entry system | Keyless entry system does not work. | E-1 |
Keyless entry hazard warning lamp answerback function or the room lamp answerback function does not work normally. | E-2 |
Encrypted code can not be registered. | E-3 |
Multimode keyless entry system function does not work at all. | E-4 |
The power windows do not work normally by means of the multimode keyless entry function. | E-5 |
The sunroof does not close normally by means of the multimode keyless entry function. | E-6 |
The timer lock function does not work after the doors have been unlocked by the keyless entry system. | E-7 |
Sunroof | The sunroof does not work at all. | F-1 |
Any of the sunroof switch positions is defective. | F-2 |
Sunroof timer function does not work normally. | F-3 |
Sunroof anti-trap function does not work normally. | F-4 |
Windshield wiper and washer | The windshield wipers do not work at all. | G-1 |
The windshield wipers do not work when the wiper switch is at "INT", "WASHER" or "MIST" position. However, the wipers work at low speed when the switch is at "LO" and "HI" position. | G-2 |
The windshield wipers do not stop at the specified park position. | G-3 |
The windshield wipers do not work normally. | G-4 |
The intermittent wiper interval can not be adjusted by operating the windshield intermittent wiper volume control. | G-5 |
The intermittent wiper interval is not changed according to the vehicle speed. | G-6 |
The windshield washer does not work. | G-7 |
Rear wiper and washer | Rear wiper do no not work at all. | H-1 |
The rear wiper does not stop at the specified park position. | H-2 |
When the selector lever is moved to "R" position during the rear wiper operation, the rear wiper does not operate at the continuous mode. | H-3 |
The rear washer does not work. | H-4 |
Electric retractable remote controlled door mirror | Electric retractable remote controlled door mirrors does not work at all. | I-1 |
Left or right side electric retractable remote controlled door mirror does not work at all. | I-2 |
Electric retractable remote controlled door mirror timer function does not work. | I-3 |
Vehicle speed-dependent unfolding function does not work normally. | I-4 |
Ignition-linked fold/unfold function does not work normally. | I-5 |
Keyless entry system-linked fold/unfold function does not work normally. | I-6 |
Ignition key cylinder illumination lamp | The ignition key cylinder illumination lamp does not illuminate/extinguish normally. | J-1 |
Headlamp and tail lamp | The tail lamps do not illuminate normally. | K-1 |
The low-beam headlamps do not illuminate normally. | K-2 |
The high-beam headlamps do not illuminate normally. | K-3 |
The high-beam and low-beam headlamps do not illuminate when the passing switch is operated. | K-4 |
The headlamp automatic shutdown function does not work normally. | K-5 |
The auto lamp function does not work normally. | K-6 |
The wiper-linked auto lamp function does not work normally. | K-7 |
Any of tail lamps, position lamps or licence plate lamp does not illuminate. <2000> | K-8 |
Any of tail lamps, position lamps or licence plate lamp does not illuminate. <2400> | K-9 |
Either of the headlamps or high-beam indicator lamps does not illuminate <Vehicles without discharge headlamp>. | K-10 |
Either of the headlamps or high-beam indicator lamps does not illuminate <Vehicles with discharge headlamp>. | K-11 |
Flasher timer | The turn-signal lamps do not illuminate. | L-1 |
The hazard warning lamps do not illuminate. | L-2 |
Any of the turn-signal lamps does not illuminate. <2000> | L-3 |
Any of the turn-signal lamps does not illuminate. <2400> | L-4 |
Fog lamp | The front fog lamps do not illuminate normally. | M-1 |
The rear fog lamps do not illuminate normally. | M-2 |
One of the front fog lamps does not illuminate. | M-3 |
Any of the rear fog lamps does not illuminate. | M-4 |
Interior lamp | The front and rear room lamp does not illuminate or extinguish normally. | N-1 |
Interior lamp automatic shutoff function does not work normally. | N-2 |
The door-ajar warning lamp does not illuminate/extinguish normally. | N-3 |
Security alarm | The security alarm is not armed. (the security alarm indicator lamp does not illuminate) | O-1 |
The interior alarm does not work normally while the security alarm is triggered. | O-2 |
The hazard warning lamps do not flash while the security alarm is triggered. | O-3 |
The horns do not sound while the security alarm is triggered. | O-4 |

[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - TROUBLE SYMPTOM CHART | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation