[37] POWER STEERING - - POWER STEERING OIL PUMP ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

POWER STEERING OIL PUMP ASSEMBLY

REMOVAL AND INSTALLATION
Pre-removal Operation Front Under Cover (RH) and Side Under Cover (RH) Removal (Refer to GROUP 51, Under Cover <2000-SOHC>, <2000-DOHC>, <2400>,). Power Steering Fluid Draining (Refer to ). | Post-installation Operation Power Steering Fluid Supplying and Bleeding (Refer to ). Drive Belt Tension Check (Refer to GROUP 11A, On-vehicle Service - Drive Belt Tension Check <2000-SOHC and 2400 (Except MIVEC)>, Refer to GROUP 11C, On-vehicle Service - Drive Belt Tensioner <2000-DOHC>, Refer to GROUP 11E, On-vehicle Service - Drive Belt Tensioner <2400 (MIVEC)>). Front Under Cover (RH) and Side Under Cover (RH) Installation (Refer to GROUP 51, Under Cover <2000-SOHC>, <2000-DOHC>, <2400>).
<2000 and 2400 (Except MIVEC)>
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Pressure switch connector
|  | 2. | Drive belt (Refer to GROUP 11A, Engine assembly <2000-SOHC and 2400 (Except MIVEC)>, Refer to GROUP 11C, Engine assembly <2000-DOHC>.)
| >>A<< | 3. | Suction hose
|  | 4. | Pressure hose
<<A>> |  | 5. | Oil pump assembly
|  | 6. | A/C compressor harness
|  | 7. | Power steering pump bracket
<2400 (MIVEC)>
|  |  | REMOVAL STEPS
--- | --- | --- | ---
|  | 1. | Drive belt (Refer to GROUP 11E, Engine assembly .)
| >>A<< | 2. | Suction hose
|  | 3. | Pressure switch connector
|  | 4. | Pressure hose
|  | 5. | Power steering oil pressure sensor harness clamp
|  | 6. | Control wiring harness clamp
|  | 7. | Battery wiring harness clamp
|  | 8. | Engine oil dipstick and dipstick guide
|  | 9. | O-ring
|  | 10. | Oil pump and bracket assembly
|  | 11. | Bracket
<<A>> |  | 12. | Oil pump assembly
| REMOVAL SERVICE POINT
| <<A>> OIL PUMP ASSEMBLY REMOVAL With the engine lifted by the jack, remove the oil pump assembly mounting bolt (lower side) at the pulley side.
| INSTALLATION SERVICE POINT
| >>A<< SUCTION HOSE INSTALLATION
| Install the suction hose so that the marking is positioned as shown in the illustration.

[37] POWER STEERING - - POWER STEERING OIL PUMP ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation