[11F] ENGINE OVERHAUL <4G69> - - FUEL AND EMISSION PARTS - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

FUEL AND EMISSION PARTS

REMOVAL AND INSTALLATION
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Throttle body
| >>C<< | 2. | Throttle body gasket
|  | 3. | Vacuum pipe and hose
|  | 4. | Solenoid valve
|  | 5. | Solenoid valve bracket
|  | 6. | Injector and delivery pipe
|  | 7. | Insulator
|  | 8. | Insulator
| >>B<< | 9. | Injector
|  | 10. | O-ring
|  | 11. | Grommet
|  | 12. | Delivery pipe
|  | 13. | EGR valve
| >>A<< | 14. | EGR gasket
| INSTALLATION SERVICE POINTS
| >>A<< EGR VALVE INSTALLATION
| Install a new gasket is positioned as shown in the illustration.
| >>B<< INJECTORS INSTALLATION
| CAUTION Use care not to let engine oil enter the delivery pipe. Apply clean engine oil to the O-ring. Insert the injector into the delivery pipe. Make sure the injector rotates smoothly. If not, remove the injector to check the O-ring for damage, and replace the O-ring if necessary. Then, reinstall the injector and check that it rotates smoothly.
| >>C<< THROTTLE BODY GASKET INSTALLATION
| Install a new gasket so that the projection is positioned as shown in the illustration.

[11F] ENGINE OVERHAUL <4G69> - - FUEL AND EMISSION PARTS - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation