[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T> - DIAGNOSTIC TROUBLE CODE PROCEDURES <4G69> - Code No.22: Input Shaft Speed Sensor System | PRINT PAGE / INDEX / PRIOR / NEXT

Code No.22: Input Shaft Speed Sensor System
OPERATION The input shaft speed sensor detects the speed of the underdrive clutch retainer, and sends the information to the engine-A/T-ECU as a pulse signal.
DIAGNOSIS CODE SET CONDITIONS The diagnosis code No.22 will be set if the input shaft speed sensor does not send a pulse signal for one second or more while the 3rd gears are engaged and the vehicle speed is 40 km/h or more (the output shaft speed sensor speed is 1000 r/min or more). If the code No.22 is set four times, the transmission will be fixed in 3rd gear as a fail-safe measure. However, the transmission can be downshifted to 2nd gear by operating the selector lever.
PROBABLE CAUSES Malfunction of input shaft speed sensor Malfunction of underdrive clutch retainer Damaged harness wires and connectors Malfunction of the engine-A/T-ECU
DIAGNOSIS PROCEDURE
STEP 1. MUT-II/III data list Item 22: Input shaft speed sensor (Refer to data list reference table ) <Except for Hong Kong spec.>. Item 01: Input shaft speed sensor (Refer to data list reference table ) <Vehicles for Hong Kong spec.>. Q: Is the check result normal? YES: Intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Go to Step 2.
STEP 2. Connector check: B-23 input shaft speed sensor connector Check for the contact with terminals. Q: Is the check result normal? YES: Go to Step 3. NO: Repair the defective connector.
STEP 3. Measure the resistance at input shaft speed sensor connector B-23. Disconnect the connector, and measure the resistance between terminal 1 and earth at the wiring harness side. OK: 2 Ω or less Q: Is the check result normal? YES: Go to Step 9. NO: Go to Step 4.
STEP 4. Measure the voltage at engine-A/T-ECU connector C-136. Connect input shaft speed sensor connector B-23. Turn the ignition switch to the ON position. Measure the voltage between engine-A/T-ECU connector C-136 terminal No.88 and earth. OK: 0.5 V or less Q: Is the check result normal? YES: Go to Step 7. NO: Go to Step 5.
STEP 5. Connector check: C-136 engine-A/T-ECU connector Check for the contact with terminals. Q: Is the check result normal? YES: Go to Step 6. NO: Repair the defective connector.
STEP 6. MUT-II/III data list Item 22: Input shaft speed sensor (Refer to data list reference table ) <Except for Hong Kong spec.>. Item 01: Input shaft speed sensor (Refer to data list reference table ) <Vehicles for Hong Kong spec.>. Q: Is the check result normal? YES: Intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the engine-A/T-ECU.
STEP 7. Connector check: C-136 engine-A/T-ECU connector, C-16 J/C (1) Check for the contact with terminals. Q: Is the check result normal? YES: Go to Step 8. NO: Repair the defective connector.
STEP 8. Check the harness between input shaft speed sensor connector B-23 terminal No.1 and engine-A/T-ECU connector C-136 terminal No.88. Check the earth line for open circuit. Q: Is the check result normal? YES: Go to Step 6. NO: Repair the wiring harness.
STEP 9. Measure the voltage at input shaft speed sensor connector B-23. Disconnect the connector, and measure the voltage between terminal 3 and earth at the wiring harness side. Turn the ignition switch to the ON position. OK: System voltage Q: Is the check result normal? YES: Go to Step 12. NO: Go to Step 10.
STEP 10. Connectors check: C-202 J/B connector, C-106 intermediate connector, C-16 J/C (1) Check for the contact with terminals. Q: Is the check result normal? YES: Go to Step 11. NO: Repair the defective connector.
STEP 11. Check the harness between input shaft speed sensor connector B-23 terminal No.3 and junction block connector C-202 terminal No.12. Check the power supply line for short or open circuit. Q: Is the check result normal? YES: Go to Step 6. NO: Repair the wiring harness.
STEP 12. Measure the voltage at input shaft speed sensor connector B-23. Disconnect the connector, and measure the voltage between terminal 2 and earth at the wiring harness side. Turn the ignition switch to the ON position. OK: 4.5 - 4.9 V Q: Is the check result normal? YES: Go to Step 18. NO: Go to Step 13.
STEP 13. Measure the voltage at engine-A/T-ECU connector C-136. Disconnect input shaft speed sensor connector B-23. Turn the ignition switch to the ON position. Measure the voltage between engine-A/T-ECU connector C-136 terminal No.64 and earth. OK: 4.5 - 4.9 V Q: Is the check result normal? YES: Go to Step 16. NO: Go to Step 14.
STEP 14. Connector check: C-136 engine-A/T-ECU connector Check for the contact with terminals. Q: Is the check result normal? YES: Go to Step 15. NO: Repair the defective connector.
STEP 15. Check the harness between input shaft speed sensor connector B-23 terminal No.2 and engine-A/T-ECU connector C-136 terminal No.64. Check the output line for short circuit. Q: Is the check result normal? YES: Go to Step 6. NO: Repair the wiring harness.
STEP 16. Connector check: C-136 engine-A/T-ECU connector Check for the contact with terminals. Q: Is the check result normal? YES: Go to Step 17. NO: Repair the defective connector.
STEP 17. Check the harness between input shaft speed sensor connector B-23 terminal No.2 and engine-A/T-ECU connector C-136 terminal No.64. Check the output line for open circuit. Q: Is the check result normal? YES: Go to Step 6. NO: Repair the wiring harness.
STEP 18. Measure the output wave pattern of the input shaft speed sensor at engine-A/T-ECU connector C-136 (using an oscilloscope). Shift the selector lever to the D range. Accelerate the vehicle to approximately 50 km/h (shift range; 3rd). Connect an oscilloscope, and measure the voltage between engine-A/T-ECU connector C-136 terminal No.64 and earth. OK: A wave pattern such as the one shown on (Check Procedure Using an Oscilloscope) should be output, and the maximum value should be 4.8 V or more and the minimum value should be 0.8 V or less. There should be no noise in the output wave pattern. Q: Is the check result normal? YES: Go to Step 6. NO: Go to Step 19.
STEP 19. Connector check: C-136 engine-A/T-ECU connector Check for the contact with terminals. Q: Is the check result normal? YES: Go to Step 20. NO: Repair the defective connector.
STEP 20. Replace the input shaft speed sensor and then recheck the diagnosis code. Replace the input shaft speed sensor. Test drive the vehicle. Check if the diagnosis code is set. Q: Is diagnosis code 22 set? YES: Go to Step 21. NO: The inspection is complete.
STEP 21. Underdrive clutch retainer inspection Visually check the underdrive clutch retainer for damage. Q: Is the check result normal? YES: Eliminate the cause of the noise. NO: Replace the underdrive clutch retainer.

[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T> - DIAGNOSTIC TROUBLE CODE PROCEDURES <4G69> - Code No.22: Input Shaft Speed Sensor System | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation