[42] BODY - - SUNROOF ASSEMBLY - SUNROOF ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

SUNROOF ASSEMBLY

REMOVAL AND INSTALLATION
Post-installation Operation <Roof lid glass assembly, Sunroof assembly> Sunroof Water Test (Refer to .) Sunroof Fit Adjustment (Refer to .) Sunroof Initializing Adjustment (Refer to .)
|  |  | Removal
--- | --- | --- | ---
|  | 1. | Deflector assembly
|  |  | Roof lid glass assembly removal steps
|  | 2. | Decoration cover
|  | 3. | Adjusting plate
|  | 4. | Roof lid glass assembly
|  |  | Sunroof switch removal steps
|  | 5. | Sunroof switch cover
|  | 6. | Sunroof switch
|  |  | Drain pipe removal steps
|  | 5. | Sunroof switch cover
|  | • | Headlining (Refer to GROUP 52A, Headlining .)
|  | • | Cowl side trim (Refer to GROUP 52A, Trims .)
| >>A<< | 7. | Drain pipe
|  |  | Sunroof motor assembly removal steps
|  | 5. | Sunroof switch cover
|  | • | Headlining (Refer to GROUP 52A, Headlining .)
|  | 8. | Sunroof motor assembly
|  |  | Sunroof assembly removal steps
|  | 5. | Sunroof switch cover
|  | 6. | Sunroof switch
|  | • | Headlining (Refer to GROUP 52A, Headlining .)
| >>A<< | 7. | Drain pipe connection
|  | 9. | Sunroof assembly
| INSTALLATION SERVICE POINTS
| >>A<< DRAIN PIPE INSTALLATION
| Install the grommet, and then position the drain pipe so that it protrudes from the grommet as shown in the illustration.

[42] BODY - - SUNROOF ASSEMBLY - SUNROOF ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation