[14] ENGINE COOLING - - ON-VEHICLE SERVICE - FAN CONTROL RELAY CONTINUITY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| FAN CONTROL RELAY CONTINUITY CHECK
Battery voltage | Terminal No. to be connected to tester | Continuity test results
--- | --- | ---
Not applied | 4 - 2 | Open circuit
Connect terminal No.1 and battery (+) terminal. Connect terminal No.3 and battery (-) terminal. | 4 - 2 | Less than 2 ohms

[14] ENGINE COOLING - - ON-VEHICLE SERVICE - FAN CONTROL RELAY CONTINUITY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation