[51] EXTERIOR - - MARK - REMOVAL AND INSTALLATION <2000> | PRINT PAGE / INDEX / PRIOR / NEXT

MARK

REMOVAL AND INSTALLATION <2000>
|  | 1. | Front three-diamond mark
| >>A<< | 2. | Rear three-diamond mark
| >>A<< | 3. | 4WD decal
| >>A<< | 4. | TURBO mark <2000 - DOHC>
| >>A<< | 5. | 20V mark
| >>A<< | 6. | AIRTREK mark <Standard - Vehicles for Hong Kong, Option - Vehicles for New Zealand>
| INSTALLATION SERVICE POINT
| >>A<< MARK INSTALLATION
| Clean the mark installation surfaces on the body with unleaded petrol. CAUTION When attaching the marks, the ambient temperature should be 20 - 38°C and the air should be completely free of dust. If the ambient temperature is lower than 20°C, the marks and the places on the vehicle body where the marks are to be attached should be heated to 20 - 38°C. Peel off the protection sheet on the back of the mark to paste it on the installation position.

[51] EXTERIOR - - MARK - REMOVAL AND INSTALLATION <2000> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation