[31] WHEEL AND TYRE - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL INFORMATION The wheels and tyres of the following specifications have been established.
SPECIFICATIONS
ROAD WHEEL AND TYRE
Item | 20V models GLX models LS models | Turbo-R models Sport-gear models GLS models XLS models | LIMITED models
--- | --- | --- | ---
Wheel | Type | Steel type or Aluminium type* | Aluminium type | Aluminium type
Size | 16 × 6JJ | 16 × 6JJ | 17 × 6.5JJ
Amount of wheel offset mm | 46 | 46 | 38
PCD mm | 114.3 | 114.3 | 114.3
Tyre | Size | 215/60 R16 95H | 215/60 R16 95H | 215/55 R17 94V
SPARE WHEEL AND TYRE
Item | Vehicles for GCC, Australia (LS, XLS models) and New Zealand (LS, XLS models) | Vehicles for Australia (LIMITED models) and New Zealand (LIMITED models) | Vehicles except for GCC, Australia and New Zealand (2400)
--- | --- | --- | ---
Spare wheel | Type | Steel type | Aluminium type | Steel type
Size | 16 × 6JJ | 17 × 6.5JJ | 16 × 4T or 16 × 6JJ*
Amount of wheel offset mm | 46 | 38 | 40 or 46*
PCD mm | 114.3 | 114.3 | 114.3
Spare tyre | Size | 215/60 R16 95H | 215/55 R17 94V | T135/90 D16 102M or 215/60 R16 95H*
NOTE: The * mark indicates optional item. NOTE: PCD (Pitch Circle Diameter) indicates the pitch circle diameter of the wheel installation holes.

[31] WHEEL AND TYRE - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation