[42] BODY - - DOOR - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

DOOR

SERVICE SPECIFICATIONS
Item | Standard value
--- | ---
Power window operation current (Power supply voltage 14.5 ± 0.5 V, at 25 °C) A | 5 ± 1
Door outside handle play mm | Front door | 0 - 3.9 (Target value: 1.9)
Rear door | 0 - 3.6 (Target value: 1.6)
Door inside handle play mm | Driver’s side | 9.3 - 17.7 (Target value: 13.9)
Except driver’s side | 3.8 - 12.2 (Target value: 8.4)
Door inside handle lock knob stroke mm | Lock side | 3 - 5
Unlock side (Front door) | 18 - 20
Unlock side (Rear side) | 17 - 19

[42] BODY - - DOOR - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation