[37] POWER STEERING - - POWER STEERING OIL PUMP ASSEMBLY - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

DISASSEMBLY AND REASSEMBLY
CAUTION Never disassemble the terminal assembly. It cannot be reassembled. <2000 and 2400 (Except MIVEC)>
|  |  | Disassembly steps
--- | --- | --- | ---
|  | 1. | Pump cover
|  | 2. | O-ring
|  | 3. | Snap ring
|  | 4. | Pulley and shaft
|  | 5. | Vanes
| >>C<< | 6. | Cam ring
|  | 7. | Rotor
|  | 8. | Pin
|  | 9. | Side plate
| >>A<< | 10. | O-ring
| >>B<< | 11. | Oil seal
|  | 12. | Terminal assembly
| >>A<< | 13. | O-ring
|  | 14. | Plug assembly
| >>A<< | 15. | O-ring
|  | 16. | Flow control spring
|  | 17. | Suction connector
| >>A<< | 18. | O-ring
<2400 (MIVEC)>
|  |  | DISASSEMBLY STEPS
--- | --- | --- | ---
|  | 1. | Pump cover
|  | 2. | O-ring
|  | 3. | Snap ring
|  | 4. | Pulley and shaft
|  | 5. | Vanes
| >>C<< | 6. | Cam ring
|  | 7. | Rotor
|  | 8. | Pin
|  | 9. | Side plate
| >>A<< | 10. | O-ring
| >>B<< | 11. | Oil seal
|  | 12. | Terminal assembly
| >>A<< | 13. | O-ring
|  | 14. | Plug assembly
| >>A<< | 15. | O-ring
|  | 16. | Flow control spring
|  | 17. | Suction connector
| >>A<< | 18. | O-ring
| REASSEMBLY SERVICE POINTS
| >>A<< O-RING INSTALLATION
No. | ID × Width mm
--- | ---
1 | 15.8 × 2.4
2 | 21.0 × 1.9
3 | 14.8 × 2.4
4 | 3.8 × 1.9
5 | 14.8 × 1.9
| >>B<< OIL SEAL INSTALLATION
| Use following special tool to install the oil seal. MB990938: Bar (Snap-in type) MB991203: Oil Seal and Bearing Installer
| >>C<< CAM RING INSTALLATION CAUTION Be sure to install the cam ring in the correct direction as shown.
| Install the cam ring as shown in the illustration.

[37] POWER STEERING - - POWER STEERING OIL PUMP ASSEMBLY - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation