[5] SYNTHETIC-RESIN PARTS - - LOCATION OF SYNTHETIC-RESIN PARTS | PRINT PAGE / INDEX / PRIOR / NEXT

LOCATION OF SYNTHETIC-RESIN PARTS The location and material of each of the principal synthetic-resin parts are shown below.
<2000>
No. | Part name | Material | Abbreviation of material | Heat-resistant temperature (°C)
--- | --- | --- | --- | ---
1 | Radiator grille | Acrylonitrile butadiene styrene | ABS | 80
2 | Door mirror
3 | Front roof rail cover
4 | Rear roof rail cover
5 | Roof spoiler
6 | Headlamp | Polycarbonate | PC | 120
7 | Tailgate handle | Polycarbonate+Polyethylene | PC+PET | 120
8 | Rear door outside handle
9 | Front door outside handle
10 | Rear splash shield | Polyethylene | PE | 100
11 | Front splash shield
12 | Rear wiper arm | Polyethylene terephthalate | PET | 115
13 | Delta cover inner | Polypropylene | PP | 80
14 | Inside rear view mirror
15 | Quarter trim lower
16 | Tailgate trim
17 | Tailgate upper trim
18 | Tailgate side trim
19 | Tailgate lower trim
20 | Rear end trim
21 | Luggage floor centre lid
22 | Luggage floor centre box
23 | Rear scuff plate
24 | Front scuff plate
25 | Cowl side trim
26 | Luggage floor side box | Polypropylene foam | PP-FOAM | 80
27 | Front bumper grille | Rubber denatured polypropylene | PP+E/P | 80
28 | Front bumper face
29 | Rear bumper face
30 | Side sill garnish
31 | Front door trim | Talc filled polypropylene (10%) | PP-TD10 (PPF) | 100-120
32 | Centre pillar trim lower
33 | Rear door trim
34 | Front deck garnish | Talc filled polypropylene (20%) | PP-TD20 (PPF) | 120-130
35 | Instrument panel
36 | Front pillar trim
37 | Centre pillar trim upper
38 | Quarter trim upper
39 | Floor console
40 | Instrument panel centre console
41 | Instrument panel console side cover
42 | Hood air inlet garnish (DOHC) |  | PPE+PA (PA+PPO) | 185
NOTE: If the material symbols designated by the ISO differ from the old symbols, both are given, with the old symboling enclosed in brackets. ISO: International Standardization Organization. A slash (/) in the material symbol indicates that two different materials make two-layer construction. A plus sign (+) indicates that the two different materials mix each other. The indicated heat-withstand temperature for parts which are composed of two or more types of material is the value for the material with the lowest heat-withstand temperature. The material symbols for synthetic-resin parts are embossed on the parts in hidden places.
<2400>
No. | Part name | Material | Abbreviation of material | Heat-resistant temperature (°C)
--- | --- | --- | --- | ---
1 | Radiator grille outer | Acrylonitrile butadiene styrene | ABS | 80
2 | Door mirror (Colour)
3 | Roof spoiler
4 | Tailgate garnish
5 | Radiator grille inner | Acrylonitrile styrene acrylate | ASA (AAS) | 80
6 | Door mirror (Black)
7 | Front roof rail cover
8 | Centre roof rail cover
9 | Rear roof rail cover
10 | Headlamp | Polycarbonate | PC | 120
11 | Rear door outside handle | Polycarbonate+Polyethylene terephthalate | PC+PET | 120
12 | Front door outside handle
13 | Front splash shield | Polyethylene | PE | 100
14 | Rear splash shield
15 | Rear wiper arm | Polyethylene terephthalate | PET | 115
16 | Front bumper core | Polypropylene | PP | 80
17 | Rear bumper core
18 | Air intake bezel
19 | Delta cover inner
20 | Inside rear view mirror
21 | Quarter trim lower
22 | Tailgate upper trim
23 | Tailgate trim
24 | Tailgate side trim
25 | Tailgate lower trim
26 | Rear end trim
27 | Luggage floor centre lid
28 | Luggage floor centre box
29 | Rear scuff plate
30 | Front scuff plate
31 | Cowl side trim
32 | Luggage floor side box | Polypropylene foam | PP-E | 80
33 | Centre cover | Rubber denatured polypropylene | PP+E/P | 80
34 | Front bumper face
35 | Rear bumper extension
36 | Rear over fender
37 | Rear door over fender
38 | Side sill garnish
39 | Front over fender
40 | Front bumper extension
41 | Rear bumper face | Talc filled rubber modified polypropylene | PP+E/P-TD(HMPP) | 80-100
42 | Front door trim | Talc filled polypropylene (10%) | PP-TD10 (PPF) | 100-120
43 | Centre pillar trim, lower
44 | rear door trim
45 | Front deck garnish | Talc filled polypropylene (20%) | PP-TD20 (PPF) | 120-130
46 | Front pillar trim
47 | Centre pillar trim upper
48 | Quarter trim upper
49 | Floor console rear
50 | Floor console panel
51 | Floor console front
52 | Lower side cover
53 | Instrument panel
NOTE: If the material symbols designated by the ISO differ from the old symbols, both are given, with the old symboling enclosed in brackets. ISO: International Standardization Organization. A slash (/) in the material symbol indicates that two different materials make two-layer construction. A plus sign (+) indicates that the two different materials mix each other. The indicated heat-withstand temperature for parts which are composed of two or more types of material is the value for the material with the lowest heat-withstand temperature. The material symbols for synthetic-resin parts are embossed on the parts in hidden places.

[5] SYNTHETIC-RESIN PARTS - - LOCATION OF SYNTHETIC-RESIN PARTS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation