[36] PARKING BRAKES - - PARKING BRAKE PEDAL <R.H. drive vehicles> - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

PARKING BRAKE PEDAL <R.H. drive vehicles>

REMOVAL AND INSTALLATION
Pre-removal Operation Console side cover <driver's side> removal (Refer to GROUP 52A, Instrument Panel Assembly ). Foot duct <driver's side> removal (Refer to GROUP 55A, Heater unit, Heater Core, Heater Blower Assembly and Evaporator Unit ). | Post-installation Operation Foot duct <driver's side> installation (Refer to GROUP 55A, Heater unit, Heater Core, Heater Blower Assembly and Evaporator Unit ). Console side cover <driver's side> installation (Refer to GROUP 52A, Instrument Panel Assembly ). Parking Brake Pedal Stroke Adjustment (Refer to ).
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Adjusting nut
|  | 2. | Nut holder
|  | 3. | Parking brake pedal assembly
|  | 4. | Sealer
|  | 5. | Pedal pad
|  | 6. | Parking brake switch
| >>A<< | 7. | Tension spring
|  | 8. | Stopper
|  | 9. | Parking brake pedal assembly
| INSTALLATION SERVICE POINT
| >>A<< TENSION SPRING INSTALLATION
| Apply grease to the mating surface of the tension spring and pedal, and then install the spring as shown.

[36] PARKING BRAKES - - PARKING BRAKE PEDAL <R.H. drive vehicles> - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation