[3] WELDED PANEL REPLACEMENT - - QUARTER OUTER | PRINT PAGE / INDEX / PRIOR / NEXT

QUARTER OUTER
CAUTION When repairing the area using foam materials do not use firing tools since the foaming materials may burn.
| NOTE ON REPAIR WORK
| INSTALLATION
| Cut only the side outer panel from 50 mm above the cut area of the gate pillar.
| Since it is not possible to fill the rear pillar with foam materials, apply urethane foam to bury the inside of the rear pillar.
| To prevent the foam materials from dripping, apply urethane foam to bury the inside of the wheel house arch. When assembling the quarter outer panel, apply in advance body sealant to the areas shown in the figure of the instructions.
| Assemble the quarter outer panel, bolt and tape the hole and flange with aluminum tape, then fill the hole with foam materials as shown in the figure of the instructions. Foam: 3M ULTRAPRO Panel foam-Yellow
| Wait 2 hours after filling the foam materials to remove the bolt and aluminium tape. Then melt the foam materials with a soldering gun so that a clip, etc. can thoroughly be inserted in the hole that was clogged with foam materials, to bore open the hole.
| After assembling the quarter outer panel it is not possible to fill the inside of the gate pillar with foam materials. Thus, push in urethane foam (L130 mm x W65 mm x H60 mm) from the hole up to the dotted line to bury the inside of the gate pillar, as shown in the figure of the instructions.

[3] WELDED PANEL REPLACEMENT - - QUARTER OUTER | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation