[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - DIAGNOSTIC TROUBLE CODE PROCEDURES - Diagnosis code 92: Side Impact Sensor (LH) System for Fault 1 diagnosis code 95: Side Impact Sensor (RH) System for Fault 1 | PRINT PAGE / INDEX / PRIOR / NEXT

Diagnosis code 92: Side Impact Sensor (LH) System for Fault 1 diagnosis code 95: Side Impact Sensor (RH) System for Fault 1
DIAGNOSIS CODE SET CONDITIONS These diagnosis codes are set if the followings are detected from the analog G-sensor inside the side impact sensor output. Analog G-sensor is not operating. Analog G-sensor characteristics are abnormal. Analog G-sensor inside the side impact sensor output is abnormal.
PROBABLE CAUSE Malfunction of side impact sensor (LH) (for diagnosis code 92) and side impact sensor (RH) (for diagnosis code 95)
| DIAGNOSIS PROCEDURE
| Replace side impact sensor (LH) (for diagnosis code 92) and side impact sensor (RH) (for diagnosis code 95). (Refer to ). Check the diagnosis code. Q: Is any of diagnosis code 92 or 95 set? YES: Replace the SRS-ECU (Refer to ). NO: The procedure is complete.

[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - DIAGNOSTIC TROUBLE CODE PROCEDURES - Diagnosis code 92: Side Impact Sensor (LH) System for Fault 1 diagnosis code 95: Side Impact Sensor (RH) System for Fault 1 | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation