[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A10. CHECK ENGINE COOLANT LEVEL IN RESERVOIR | PRINT PAGE / INDEX / PRIOR / NEXT

| A10. CHECK ENGINE COOLANT LEVEL IN RESERVOIR
| Check that the coolant level is between the "FULL" and "LOW" lines when the engine is at the normal operating temperature.

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A10. CHECK ENGINE COOLANT LEVEL IN RESERVOIR | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation