[54C] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Hong Kong spec.> - - SYMPTOM PROCEDURES - TONE ALARM - INSPECTION PROCEDURE B-2: Lamp reminder buzzer function does not work normally. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE B-2: Lamp reminder buzzer function does not work normally.
| CAUTION Whenever the ECU is replaced, ensure that the input and output signal circuits are normal.
| COMMENTS ON TROUBLE SYMPTOM The ETACS-ECU operates this function in accordance with the input signals below. Ignition switch (IG1) Driver's door switch Tail lamp switch Headlamp switch If this function does not work normally, these input signal circuit(s) or the ETACS-ECU may be defective.
| POSSIBLE CAUSES Malfunction of the driver's door switch Malfunction of the column switch Malfunction of the ETACS-ECU Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. ECU check on the SWS monitor Check that the power supply and earth lines to the ETACS-ECU and the column switch (column-ECU) and the SWS communication lines are normal. Ignition switch: OFF ECUS TO BE CHECKED ETACS ECU COLUMN ECU OK: "OK" are displayed for all the items Q: Are the check result normal? "OK" are displayed for all the items: Go to Step 2. "NG" is displayed on the "ETACS ECU" menu.: Refer to Inspection Procedure A-3 "Communication with the ETACS-ECU is not possible" . "NG" is displayed on the "COLUMN ECU" menu.: Refer to Inspection Procedure A-2 "Communication with the column switch (column-ECU) is not possible" .
| Step 2. Function diagnosis by using the SWS monitor Check the SWS communication signal, which are related to the lamp reminder function. <Selected item> BUZZER - LGT MONI.ALRM Ignition switch: OFF (key removed) Lighting switch: HEAD Driver's door: open
Item No. | Item name | Normal conditions
--- | --- | ---
Item 00 | HEADLAMP SW | ON
Item 01 | TAIL LAMP SW | ON
Item 30 | IG SW(IG1) | OFF
Item 32 | DR DOOR SW | ON
Item 43 | BUZZER | ON
OK: Normal conditions are displayed for all the items. Q: Are the check result normal? Normal conditions displayed for all the items: Go to Step 3. Normal condition is not displayed for item No.00: Refer to inspection procedure P-5 "The column switch (lighting and turn-signal lamp switch) signal is not received" . Normal condition is not displayed for item No.01: Refer to inspection procedure P-5 "The column switch (lighting and turn-signal lamp switch) signal is not received" . Normal condition is not displayed for item No.30: Refer to inspection procedure P-2 "The ignition switch (IG1) signal is not received" . Normal condition is not displayed for item No.32: Refer to inspection procedure P-4 "The driver's door switch signal is not received" . Normal condition is not displayed for item No.43: Replace the ETACS-ECU.
| Step 3. Retest the system. The lamp reminder buzzer function should work normally. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the ETACS-ECU.

[54C] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Hong Kong spec.> - - SYMPTOM PROCEDURES - TONE ALARM - INSPECTION PROCEDURE B-2: Lamp reminder buzzer function does not work normally. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation