[1] PRE-DELIVERY INSPECTION - - BODY - 4. OPERATION OF DOOR LOCKING SYSTEMS AND DOOR HINGES | PRINT PAGE / INDEX / PRIOR / NEXT

| 4. OPERATION OF DOOR LOCKING SYSTEMS AND DOOR HINGES
| Open each door to check the release mechanism and ease of operation. Close the door to check the latch and striker. Open the door, operate the lock lever and close the door to check the lock. Partially close the door to check the open-door detent. Unlock each door with the key to check lock operation. Verify that all doors can be locked by the lock buttons. NOTE: Adjust and lubricate the door latches, strikers and locks as required.
| Verify that the rear doors can't be opened by the inner door handle when the child protection knob at the end of the door is shifted to the "LOCK" position with the inside lock plunger raised. CAUTION Set the lock to the "FREE" position on child protection of both rear doors. (For four door models)

[1] PRE-DELIVERY INSPECTION - - BODY - 4. OPERATION OF DOOR LOCKING SYSTEMS AND DOOR HINGES | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation