[35A] SERVICE BRAKE - - REAR BRAKE | PRINT PAGE / INDEX / PRIOR / NEXT

REAR BRAKE
REAR DRUM BRAKE <EXCEPT FOR HONG KONG SPEC. (2000-DOHC AND 2400), SOUTH AFRICA AND ARGENTINA> 9-inch leading trailing-type drum brakes have been adopted for the rear brakes in order to provide stable braking force at all times both when moving forward and reversing.
REAR DISC BRAKE <VEHICLES FOR HONG KONG SPEC. (2000-DOHC AND 2400), SOUTH AFRICA, ARGENTINA AND NEW ZEALAND (2400)> Brakes with the following specifications have been adopted for the rear brakes. S4-S38 1-piston solid discs* . An outer disc method in which the wheels and discs are tightened together has been adopted to improve the ease of brake disc removal and installation. The brake pads are equipped with mechanical-type audible wear indicators to notify the driver when the usage limit (2 mm) has been reached. NOTE: * For the brake disc name, refer to FRONT BRAKE .

[35A] SERVICE BRAKE - - REAR BRAKE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation