[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - TROUBLESHOOTING - PULSE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| PULSE CHECK
| CAUTION Before connecting or disconnecting the MUT-II/III, turn the ignition switch to the "LOCK" (OFF) position. The input signals (signals other than communication line signals), which are compatible with the SWS monitor by using the MUT-II/III or voltmeter, can be confirmed by the Pulse Check. NOTE: If a problem is found in the "Pulse Check", refer to the Problems during Input Signal Check <Service data, function diagnosis or pulse check> (Refer to ). Use the MUT-II/III or voltmeter to check the following input signals.
| SWITCHES WHICH ARE APPLICABLE TO INPUT SIGNAL CHECK, AND THEIR CHECK CONDITIONS
Input signal | Requirements for sounding buzzer
--- | ---
Key reminder switch <vehicles with keyless entry system> | When the inserted ignition key is pulled out.
Hazard warning lamp switch | When the switch is turned from off to on.
Front fog lamp switch
Rear fog lamp switch
All of the door switches | A door is opened when all the doors are closed.
Driver's door lock actuator | When the driver's key cylinder or inside lock knob is unlocked or locked.
Vehicle speed signal (engine-A/T-ECU) <Except vehicles for GCC> | When the vehicle speed has reached 10 km/h or more.
Keyless entry transmitter | Switches | When the switch is turned from off to on.
Interior lamp loaded signal | When a load is applied through multi-purpose fuse No.22.

[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - TROUBLESHOOTING - PULSE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation