[54A] CHASSIS ELECTRICAL - - HORN - HORN TROUBLESHOOTING <vehicles with theft alarm system> | PRINT PAGE / INDEX / PRIOR / NEXT

HORN

HORN TROUBLESHOOTING <vehicles with theft alarm system>
The theft-alarm system horn is controlled by the Smart Wiring System (SWS). For troubleshooting, refer to respective Groups below. Not using SWS monitor <Hong Kong spec.>: GROUP 54B, Troubleshooting . Using SWS monitor <Hong Kong spec.>: GROUP 54C, Troubleshooting . Not using SWS monitor <Except for Hong Kong spec.>: GROUP 54D, Troubleshooting . Using SWS monitor <Except for Hong Kong spec.>: GROUP 54E, Troubleshooting .

[54A] CHASSIS ELECTRICAL - - HORN - HORN TROUBLESHOOTING <vehicles with theft alarm system> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation