[54A] CHASSIS ELECTRICAL - - CIGARETTE LIGHTER - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

CIGARETTE LIGHTER

| INSPECTION
| CIGARETTE LIGHTER CHECK
| Take out the plug, and check for a worn edge on the element spot connection, and for shreds of tobacco or other material on the element. Using an ohmmeter, check that the element resistance value is 1.7 ohms.

[54A] CHASSIS ELECTRICAL - - CIGARETTE LIGHTER - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation