[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - ON-VEHICLE SERVICE - FUEL PUMP CONNECTOR DISCONNECTION (HOW TO REDUCE PRESSURIZED FUEL LINES) | PRINT PAGE / INDEX / PRIOR / NEXT

| FUEL PUMP CONNECTOR DISCONNECTION (HOW TO REDUCE PRESSURIZED FUEL LINES) WARNING When removing the fuel pipe, etc., release fuel pressure to prevent fuel spray. Remove the rear seat assembly (Refer to GROUP 52A - Rear Seat Assembly ).
| Remove the service hole cover.
| Disconnect the fuel pump assembly connector <2WD> or fuel tank pump and gauge assembly connector <4WD>. After starting the engine and letting it run until it stops naturally, turn the ignition switch to the "LOCK" (OFF) position. Connect the fuel pump assembly connector <2WD> or fuel tank pump and gauge assembly connector <4WD>. Install the service hole cover and rear seat assembly (Refer to GROUP 52A - Rear Seat Assembly ).

[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - ON-VEHICLE SERVICE - FUEL PUMP CONNECTOR DISCONNECTION (HOW TO REDUCE PRESSURIZED FUEL LINES) | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation