[13B] MULTIPORT FUEL INJECTION (MPI) <4G64> - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
Items | Specifications
--- | ---
Basic idle speed r/min | 700 ± 50
Throttle position sensor adjusting voltage mV | 535 - 735
Throttle position sensor resistance kΩ | 3.5 - 6.5
Idle speed control servo coil resistance (at 20°C) Ω | 26 - 33
Intake air temperature sensor resistance kΩ | -20°C | 13 - 17
0°C | 5.3 - 6.7
20°C | 2.3 - 3.0
40°C | 1.0 - 1.5
60°C | 0.56 - 0.76
80°C | 0.30 - 0.42
Engine coolant temperature sensor resistance kΩ | -20°C | 14 - 17
0°C | 5.1 - 6.5
20°C | 2.1 - 2.7
40°C | 0.9 - 1.3
60°C | 0.48 - 0.68
80°C | 0.26 - 0.36
Fuel pressure kPa | Vacuum hose disconnection | 330 - 350 at curb idle
Vacuum hose connection | Approximately 270 at curb idle
Injector coil resistance (at 20°C) Ω | 13 - 16
Mixture adjusting screw (Variable resistor) resistance kΩ | 3.5 - 6.5

[13B] MULTIPORT FUEL INJECTION (MPI) <4G64> - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation