[15] INTAKE AND EXHAUST - - ON-VEHICLE SERVICE - WASTE GATE SOLENOID VALVE CHECK <Turbo> | PRINT PAGE / INDEX / PRIOR / NEXT

| WASTE GATE SOLENOID VALVE CHECK <Turbo>
| OPERATION CHECK
| Connect a hand vacuum pump to the solenoid valve nipple A. Using a jumper wire, connect between the solenoid valve terminal and battery terminal. Connecting and disconnecting the jumper wire at the battery negative terminal to apply a negative pressure, check tightness.
Jumper wire | B nipple condition | Normal condition
--- | --- | ---
Connected | Opened | Negative pressure leaks.
Closed | Negative pressure is held.
Disconnected | Opened | Negative pressure is held.
| COIL RESISTANCE CHECK
| Measure the resistance between solenoid valve terminals Standard value: 29 - 35 Ω (at 20°C)

[15] INTAKE AND EXHAUST - - ON-VEHICLE SERVICE - WASTE GATE SOLENOID VALVE CHECK <Turbo> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation