[55B] AUTOMATIC AIR CONDITIONER - - TROUBLESHOOTING - ACTUATOR TEST TABLE | PRINT PAGE / INDEX / PRIOR / NEXT

ACTUATOR TEST TABLE
Item No. | Check items | Drive content
--- | --- | ---
01 | Blower motor | Stop
02 | Low speed
03 | Middle speed
04 | High speed
05 | Motor for Air mixing door | Open angle: Approximately 0% (MAX COOL)
06 | Opening angle: approximately 50%
07 | Open angle: Approximately 100% (MAX HOT)
08 | Motor for mode selection damper | FACE
09 | FOOT
10 | DEF
11 | Compressor output | OFF
12 | ON
13 | Motor for outside/inside air selection damper | Outside air
14 | Inside air
38 | Idle-up | OFF (A/C high pressure)
39 | ON (A/C low pressure)

[55B] AUTOMATIC AIR CONDITIONER - - TROUBLESHOOTING - ACTUATOR TEST TABLE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation