[26] FRONT AXLE - - FRONT AXLE HUB ASSEMBLY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION Check the hub for cracks and spline for wear. Check the knuckle for cracks. Check for defective bearing. NOTE: If the meshing of the wheel bearing outer race and the knuckle, or of the wheel bearing inner race and the hub, is loose, replace the bearing or damaged parts.

[26] FRONT AXLE - - FRONT AXLE HUB ASSEMBLY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation