[55B] AUTOMATIC AIR CONDITIONER - - COMPRESSOR ASSEMBLY AND TENSION PULLEY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| COMPRESSOR MAGNETIC CLUTCH OPERATION CHECK
| Connect the compressor connector terminal to the battery positive (+) terminal and earth the battery’s negative (-) terminal to the compressor unit. At that time, the magnetic clutch should make a definite operating sound.

[55B] AUTOMATIC AIR CONDITIONER - - COMPRESSOR ASSEMBLY AND TENSION PULLEY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation