[16] ENGINE ELECTRICAL - - IGNITION SYSTEM - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
IGNITION COIL <4G6-SOHC, 4G6DOHC>
Item | Standard value
--- | ---
Secondary coil resistance kΩ | 8.5 - 11.5
SPARK PLUG
Item |  | Standard value | Limit
--- | --- | --- | ---
Spark plug gap mm | 4G63-DOHC | 0.7 - 0.8 | 1.0
4G63-SOHC | 1.0 - 0.1 | -
4G64-SOHC | 0.7 - 0.8 | -
4G69-MIVEC | 0.7 - 0.8 | 1.2
RESISTIVE CORD <4G6-SOHC, 4G6-DOHC>
Item | Standard value | Limit
--- | --- | ---
Resistance kΩ | - | Maximum 19

[16] ENGINE ELECTRICAL - - IGNITION SYSTEM - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation