[15] INTAKE AND EXHAUST - - EXHAUST PIPE AND MAIN MUFFLER - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

EXHAUST PIPE AND MAIN MUFFLER

REMOVAL AND INSTALLATION
<4G63-SOHC>
|  |  | Exhaust main muffler removal steps
--- | --- | --- | ---
|  | 1. | Exhaust main muffler
|  | 4. | Exhaust pipe gasket
|  | 5. | Hanger
|  |  | Centre exhaust pipe removal steps
|  | 2. | Centre exhaust pipe
|  | 4. | Exhaust pipe gasket
|  | 6. | Exhaust pipe gasket
|  | 7. | Hanger
|  |  | Front exhaust pipe removal steps
|  | • | Centre under cover (front) (Refer to GROUP 51, Under Cover ).
|  | 3. | Front exhaust pipe
|  | 8. | Exhaust pipe gasket
|  | 9. | Exhaust pipe gasket
|  | 10. | Hanger
<4G63-DOHC>
|  |  | Exhaust main muffler removal steps
--- | --- | --- | ---
|  | 1. | Exhaust main muffler
|  | 4. | Exhaust pipe gasket
|  | 5. | Hanger
|  | 6. | Exhaust pipe damper
|  |  | Centre exhaust pipe removal steps
|  | 2. | Centre exhaust pipe
|  | 4. | Exhaust pipe gasket
|  | 7. | Exhaust pipe gasket
|  | 8. | Exhaust pipe damper
|  |  | Front exhaust pipe removal steps
|  | • | Centre under cover (front) (Refer to GROUP 51, Under Cover ).
|  | 3. | Front exhaust pipe
|  | 9. | Exhaust pipe gasket
|  | 10. | Seal ring
|  | 11. | Hanger
<4G64-SOHC>
|  |  | Exhaust main muffler removal steps
--- | --- | --- | ---
|  | 1. | Exhaust main muffler
|  | 5. | Exhaust pipe gasket
|  | 6. | Hanger
|  | 7. | Exhaust pipe damper
|  |  | Centre exhaust pipe removal steps
|  | 2. | Centre exhaust pipe
|  | 5. | Exhaust pipe gasket
|  | 8. | Exhaust pipe gasket
|  | 9. | Hanger
|  |  | Pre muffler removal steps
|  | 3. | Pre muffler
|  | 8. | Exhaust pipe gasket
|  | 10. | Exhaust pipe gasket
|  |  | Front exhaust pipe removal steps
|  | • | Centre under cover (front) (Refer to GROUP 51, Under Cover ).
|  | 4. | Front exhaust pipe
|  | 10. | Exhaust pipe gasket
|  | 11. | Exhaust pipe gasket
|  | 12. | Hanger
|  | 13. | Front exhaust pipe bracket
<4G69>
|  |  | Exhaust main muffler removal steps
--- | --- | --- | ---
|  | 1. | Exhaust main muffler
|  | 5. | Exhaust pipe gasket
|  | 6. | Hanger
|  | 7. | Exhaust pipe damper
|  |  | Centre exhaust pipe removal steps
|  | 2. | Centre exhaust pipe
|  | 5. | Exhaust pipe gasket
|  | 8. | Exhaust pipe gasket
|  | 9. | Hanger
|  |  | Front exhaust pipe removal steps
|  | • | Centre under cover (front) (Refer to GROUP 51, Under Cover ).
<<A>> | >>A<< | 3. | Oxygen sensor <Vehicles for Hong Kong, Brunei, Singapore, Malaysia>
|  | 4. | Front exhaust pipe
|  | 10. | Exhaust pipe gasket
|  | 11. | Exhaust pipe gasket
|  | 12. | Hanger
| REMOVAL SERVICE POINT
| <<A>> OXYGEN SENSOR REMOVAL
| Use special tool oxygen sensor wrench (MD998770) to remove the oxygen sensor.
| INSTALLATION SERVICE POINT
| >>A<< OXYGEN SENSOR INSTALLATION
| Use special tool oxygen sensor wrench (MD998770) to install the oxygen sensor.

[15] INTAKE AND EXHAUST - - EXHAUST PIPE AND MAIN MUFFLER - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation