[11F] ENGINE OVERHAUL <4G69> - - ALTERNATOR AND IGNITION SYSTEM - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

ALTERNATOR AND IGNITION SYSTEM

REMOVAL AND INSTALLATION
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Oil level gauge
|  | 2. | Oil level gauge guide
|  | 3. | O-ring
|  | 4. | Auto tensioner
|  | 5. | Crankshaft pulley
|  | 6. | Water pump pulley
|  | 7. | Idler pulley
|  | 8. | Connector bracket
|  | 9. | Alternator
|  | 10. | Ignition coil
<<A>> | >>C<< | 11. | Spark plug
|  | 12. | Connector bracket
|  | 13. | Camshaft position sensor
|  | 14. | O-ring
| >>B<< | 15. | Camshaft position sensor support
<<B>> | >>A<< | 16. | Camshaft position sensing cylinder
| REMOVAL SERVICE POINT
| <<A>> SPARK PLUG REMOVAL
| Using special tool Spark plug wrench (MB991398), removal the spark plug.
| <<B>> CAMSHAFT POSITION SENSING CYLINDER REMOVAL
| Using special tool Fly wheel stopper (MD998781), hold the drive plate. Removal the camshaft position sensing cylinder.
| INSTALLATION SERVICE POINT
| >>A<< CAMSHAFT POSITION SENSING CYLINDER INSTALLATION
| Using special tool Fly wheel stopper (MD998781), hold the drive plate. Tighten the camshaft position sensing cylinder to the specified torque. Tightening torque: 22 ± 4 N·m
| >>B<< CAMSHAFT POSITION SENSOR SUPPORT INSTALLATION
| Remove completely the FIPG remaining on the camshaft position sensor support and cylinder head. Apply a 3 ± 1 mm diameter bead of FIPG to the indicated surface of the camshaft position sensor support. Specified sealant: Mitsubishi Genuine Part No.MD970389 or equivalent
| >>C<< SPARK PLUG INSTALLATION
| Using special tool Spark plug wrench (MB991398), tighten the spark plug to the specified torque. Tightening torque: 25 ± 5 N·m

[11F] ENGINE OVERHAUL <4G69> - - ALTERNATOR AND IGNITION SYSTEM - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation