[1] PRE-DELIVERY INSPECTION - - BEFORE ROAD TEST - 18. INHIBITOR SWITCH | PRINT PAGE / INDEX / PRIOR / NEXT

| 18. INHIBITOR SWITCH On models with an automatic transmission, be sure the engine starts in both "P" and "N" position, and does not start in other positions.

[1] PRE-DELIVERY INSPECTION - - BEFORE ROAD TEST - 18. INHIBITOR SWITCH | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation