[55B] AUTOMATIC AIR CONDITIONER - - TROUBLESHOOTING - DATA LIST REFERENCE TABLE | PRINT PAGE / INDEX / PRIOR / NEXT

DATA LIST REFERENCE TABLE
Item No. | Check items | Inspection conditions | Normal condition
--- | --- | --- | ---
11 | Interior temperature sensor | Ignition switch: ON | Room temperature is the same as MUT-II displayed temperature.
13 | Outside air temperature sensor | Ignition switch: ON | Outside temperature is the same as MUT-II displayed temperature.
15 | Heater water temperature sensor | Ignition switch: ON | Heater core wall surface temperature is the same as MUT-II displayed temperature.
21 | Air thermo sensor | Ignition switch: ON | Evaporator outlet temperate is the same as MUT-II displayed temperature
25 | Photo sensor | Ignition switch: ON Change the volume of insolation. | The volume of insolation takes inverse proportion with the MUT-II displayed voltage.
31 | Potentiometer for air mixing door | Ignition switch: ON Door position: MAX HOT | Opening angle: approximately 100%
Ignition switch: ON Door position: MAX COOL | Opening angle: approximately 0%
32 | Potentiometer for mode selection damper | Ignition switch: ON Damper position: FACE | Opening angle: approximately 0%
Ignition switch: ON Damper position: FOOT | Opening angle: approximately 60%
Ignition switch: ON Damper position: FOOT/DEF | Opening angle: approximately 80%
Ignition switch: ON Damper position: DEF | Opening angle: approximately 100%
42 | A/C pressure sensor | Ignition switch: ON | Refrigerant pressure is the same as MUT-II displayed pressure.

[55B] AUTOMATIC AIR CONDITIONER - - TROUBLESHOOTING - DATA LIST REFERENCE TABLE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation