[23C] AUTOMATIC TRANSMISSION OVERHAUL <W5A5> - - DIRECT PLANETARY CAREER - DISASSMEBLY AND ASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

DIRECT PLANETARY CAREER

DISASSMEBLY AND ASSEMBLY
|  |  | Disassembly steps
--- | --- | --- | ---
<<A>> | >>D<< | 1. | Lock nut
|  | 2. | Roller bearing
|  | 3. | Thrust bearing No.9
|  | 4. | Thrust race No.10
<<B>> | >>C<< | 5. | Output gear
<<B>> | >>C<< | 6. | Parking gear
<<C>> | >>B<< | 7. | Taper roller bearing
|  | 8. | Transfer driven gear and direct annulus gear
<<D>> | >>A<< | 9. | Taper roller bearing
|  | 10. | Direct planetary carrier
| DISASSEMBLY SERVICE POINTS
| <<A>> LOCK NUT REMOVAL
| Undo staking of the lock nut.
| Use the special tool Special spanner (MD998834) to remove the lock nut.
| <<B>> OUTPUT GEAR/PARKING GEAR REMOVAL
| Use the special tool Bearing remover (MD998917) to remove the output gear and parking gear.
| <<C>> TAPER ROLLER BEARING REMOVAL
| Support the transfer driven gear as shown in the illustration. Push the shaft of the direct planetary carrier to remove the taper roller bearing and gear.
| <<D>> TAPER ROLLER BEARING REMOVAL
| Use the special tool Bearing remover (MD998917) to remove the taper roller bearing.
| REASSEMBLY SERVICE POINTS
| >>A<< TAPER ROLLER BEARING INSTALLATION
| Use the special tools to install the taper roller bearing. Installer cap (MD998812) Installer 100 (MD998813) Installer adapter (MD998824)
| >>B<< TAPER ROLLER BEARING INSTALLATION
| Use the special tools to install the taper roller bearing. Installer cap (MD998812) Installer 100 (MD998813) Installer adapter (MD998824)
| >>C<< OUTPUT GEAR/PARKING GEAR INSTALLATION
| Use the special tools to install the output gear and parking gear. Installer cap (MD998812) Installer adapter (50) (MD998824)
| >>D<< LOCK NUT INSTALLATION
| Smear ATF on a new lock nut and tighten it to the specified torque of 167 ± 10 N·m, using the special tool Special spanner (MD998834). Loosen the nut one turn, then tighten it to the specified torque of 167 ± 10 N·m again.
| Use a punch to stake the lock nut at two places.

[23C] AUTOMATIC TRANSMISSION OVERHAUL <W5A5> - - DIRECT PLANETARY CAREER - DISASSMEBLY AND ASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation