[11D] ENGINE OVERHAUL <4G6-DOHC> - - OIL PAN AND OIL PUMP - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| COUNTERBALANCE SHAFTS Check that the oil holes are not blocked. Clean if necessary.
| Check the journals for seizure, damage and defective contact with bearings. If any of these faults is found, replace the counterbalance shaft, bearings and/or oil pump case assembly.
| OIL PUMP
| Install the drive and driven gears in the oil pump case. Measure the gear side clearance using a straight edge and thickness gauge. Standard values: Drive gear 0.08 - 0.14 mm Driven gear 0.06 - 0.12 mm

[11D] ENGINE OVERHAUL <4G6-DOHC> - - OIL PAN AND OIL PUMP - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation